(kicad_pcb (version 20171130) (host pcbnew 5.1.6+dfsg1-1~bpo10+1)
  (general
    (thickness 1.6002)
    (drawings 109)
    (tracks 756)
    (zones 0)
    (modules 67)
    (nets 79)
  )
  (page A4)
  (layers
    (0 Front signal)
    (31 Back signal)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (user_trace_width 0.15)
    (user_trace_width 0.2)
    (user_trace_width 0.4)
    (user_trace_width 0.6)
    (trace_clearance 0.127)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.127)
    (via_size 0.6)
    (via_drill 0.3)
    (via_min_size 0.6)
    (via_min_drill 0.3)
    (user_via 0.6 0.3)
    (user_via 0.9 0.4)
    (uvia_size 0.6858)
    (uvia_drill 0.3302)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (edge_width 0.0381)
    (segment_width 0.254)
    (pcb_text_width 0.3048)
    (pcb_text_size 1.524 1.524)
    (mod_edge_width 0.1524)
    (mod_text_size 0.8128 0.8128)
    (mod_text_width 0.1524)
    (pad_size 1.524 1.524)
    (pad_drill 1.2)
    (pad_to_mask_clearance 0)
    (solder_mask_min_width 0.12)
    (aux_axis_origin 63.5 139.7)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "gerber/"))
  )
  (net 0 "")
  (net 1 /-18V_FP)
  (net 2 /RST)
  (net 3 "Net-(C9-Pad2)")
  (net 4 "Net-(C9-Pad1)")
  (net 5 /FPREF)
  (net 6 /FIL1)
  (net 7 /FPSTBY)
  (net 8 /BFPRST)
  (net 9 /BFPDO)
  (net 10 /FIL2)
  (net 11 /+18V_FLT)
  (net 12 /BFPDI)
  (net 13 /D-)
  (net 14 "Net-(J2-Pad1)")
  (net 15 /D+)
  (net 16 /DSP_CS)
  (net 17 /DSP_DC)
  (net 18 "Net-(J3-Pad6)")
  (net 19 /DSP_DI)
  (net 20 /DSP_SCLK)
  (net 21 "Net-(J3-Pad3)")
  (net 22 /RXD)
  (net 23 "Net-(IC1-Pad3)")
  (net 24 /KP_R3)
  (net 25 /KP_C0)
  (net 26 /KP_R2)
  (net 27 /KP_R1)
  (net 28 /KP_R0)
  (net 29 /KP_C1)
  (net 30 /KP_C2)
  (net 31 /KP_C3)
  (net 32 /KP_C4)
  (net 33 /RE_A)
  (net 34 /RE_B)
  (net 35 /TXD)
  (net 36 "Net-(U2-Pad62)")
  (net 37 "Net-(U2-Pad54)")
  (net 38 "Net-(U2-Pad53)")
  (net 39 "Net-(U2-Pad52)")
  (net 40 "Net-(U2-Pad51)")
  (net 41 "Net-(U2-Pad43)")
  (net 42 "Net-(U2-Pad42)")
  (net 43 "Net-(U2-Pad41)")
  (net 44 "Net-(U2-Pad40)")
  (net 45 "Net-(U2-Pad39)")
  (net 46 "Net-(U2-Pad38)")
  (net 47 "Net-(U2-Pad37)")
  (net 48 "Net-(U2-Pad36)")
  (net 49 "Net-(U2-Pad35)")
  (net 50 "Net-(U2-Pad34)")
  (net 51 "Net-(U2-Pad33)")
  (net 52 "Net-(U2-Pad30)")
  (net 53 "Net-(U2-Pad29)")
  (net 54 /MISO)
  (net 55 "Net-(U2-Pad11)")
  (net 56 "Net-(U2-Pad4)")
  (net 57 "Net-(U2-Pad3)")
  (net 58 "Net-(U2-Pad2)")
  (net 59 "Net-(J2-Pad4)")
  (net 60 "Net-(IC1-Pad4)")
  (net 61 "Net-(C14-Pad1)")
  (net 62 "Net-(C15-Pad1)")
  (net 63 "Net-(U2-Pad28)")
  (net 64 "Net-(U2-Pad27)")
  (net 65 "Net-(R18-Pad1)")
  (net 66 /NRST)
  (net 67 "Net-(J4-Pad6)")
  (net 68 "Net-(J4-Pad5)")
  (net 69 "Net-(J4-Pad4)")
  (net 70 "Net-(J4-Pad2)")
  (net 71 /SWCLK)
  (net 72 /SWDIO)
  (net 73 /SWO)
  (net 74 GND)
  (net 75 /+3.3V)
  (net 76 /+5V)
  (net 77 /~DSP_RST)
  (net 78 "Net-(U3-Pad4)")
  (net_class Default "This is the default net class."
    (clearance 0.127)
    (trace_width 0.127)
    (via_dia 0.6)
    (via_drill 0.3)
    (uvia_dia 0.6858)
    (uvia_drill 0.3302)
    (diff_pair_width 0.1524)
    (diff_pair_gap 0.254)
    (add_net /+18V_FLT)
    (add_net /+3.3V)
    (add_net /+5V)
    (add_net /-18V_FP)
    (add_net /BFPDI)
    (add_net /BFPDO)
    (add_net /BFPRST)
    (add_net /D+)
    (add_net /D-)
    (add_net /DSP_CS)
    (add_net /DSP_DC)
    (add_net /DSP_DI)
    (add_net /DSP_SCLK)
    (add_net /FIL1)
    (add_net /FIL2)
    (add_net /FPREF)
    (add_net /FPSTBY)
    (add_net /KP_C0)
    (add_net /KP_C1)
    (add_net /KP_C2)
    (add_net /KP_C3)
    (add_net /KP_C4)
    (add_net /KP_R0)
    (add_net /KP_R1)
    (add_net /KP_R2)
    (add_net /KP_R3)
    (add_net /MISO)
    (add_net /NRST)
    (add_net /RE_A)
    (add_net /RE_B)
    (add_net /RST)
    (add_net /RXD)
    (add_net /SWCLK)
    (add_net /SWDIO)
    (add_net /SWO)
    (add_net /TXD)
    (add_net /~DSP_RST)
    (add_net GND)
    (add_net "Net-(C14-Pad1)")
    (add_net "Net-(C15-Pad1)")
    (add_net "Net-(C9-Pad1)")
    (add_net "Net-(C9-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(J2-Pad1)")
    (add_net "Net-(J2-Pad4)")
    (add_net "Net-(J3-Pad3)")
    (add_net "Net-(J3-Pad6)")
    (add_net "Net-(J4-Pad2)")
    (add_net "Net-(J4-Pad4)")
    (add_net "Net-(J4-Pad5)")
    (add_net "Net-(J4-Pad6)")
    (add_net "Net-(R18-Pad1)")
    (add_net "Net-(U2-Pad11)")
    (add_net "Net-(U2-Pad2)")
    (add_net "Net-(U2-Pad27)")
    (add_net "Net-(U2-Pad28)")
    (add_net "Net-(U2-Pad29)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad30)")
    (add_net "Net-(U2-Pad33)")
    (add_net "Net-(U2-Pad34)")
    (add_net "Net-(U2-Pad35)")
    (add_net "Net-(U2-Pad36)")
    (add_net "Net-(U2-Pad37)")
    (add_net "Net-(U2-Pad38)")
    (add_net "Net-(U2-Pad39)")
    (add_net "Net-(U2-Pad4)")
    (add_net "Net-(U2-Pad40)")
    (add_net "Net-(U2-Pad41)")
    (add_net "Net-(U2-Pad42)")
    (add_net "Net-(U2-Pad43)")
    (add_net "Net-(U2-Pad51)")
    (add_net "Net-(U2-Pad52)")
    (add_net "Net-(U2-Pad53)")
    (add_net "Net-(U2-Pad54)")
    (add_net "Net-(U2-Pad62)")
    (add_net "Net-(U3-Pad4)")
  )
  (module Symbol:OSHW-Symbol_13.4x12mm_SilkScreen (layer Back) (tedit 0)
    (at 92.202 95.5548 180)
    (descr "Open Source Hardware Symbol")
    (tags "Logo Symbol OSHW")
    (attr virtual)
    (fp_text reference REF** (at 0 0) (layer B.SilkS) hide)
    (fp_text value OSHW-Symbol_13.4x12mm_SilkScreen (at 0.75 0) (layer B.Fab) hide)
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 197 109.2)
    (fp_text reference SW16 (at 0 -4.171) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 28 /KP_R0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 31 /KP_C3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module Package_TO_SOT_SMD:SOT-23-5 (layer Front) (tedit 5A02FF57)
    (at 188.722 75.522 270)
    (descr "5-pin SOT23 package")
    (tags SOT-23-5)
    (attr smd)
    (fp_text reference U3 (at -3.1955 0.0635 180) (layer F.SilkS))
    (fp_text value MCP1811AT-033_OT (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 75 /+3.3V))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 78 "Net-(U3-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 76 /+5V))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 74 GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 76 /+5V))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-5.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hp34970:SOP65P640X120-14N (layer Front) (tedit 5F665E8C)
    (at 140.9065 79.5655 180)
    (fp_text reference U1 (at -0.595 -3.435) (layer F.SilkS))
    (fp_text value LSF0204PWR (at 7.025 3.435) (layer F.Fab))
    (pad 1 smd rect (at -2.87 -1.95 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 75 /+3.3V))
    (pad 2 smd rect (at -2.87 -1.3 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 35 /TXD))
    (pad 3 smd rect (at -2.87 -0.65 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 22 /RXD))
    (pad 4 smd rect (at -2.87 0 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 2 /RST))
    (pad 5 smd rect (at -2.87 0.65 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 74 GND))
    (pad 6 smd rect (at -2.87 1.3 180) (size 1.57 0.41) (layers Front F.Paste F.Mask))
    (pad 7 smd rect (at -2.87 1.95 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 74 GND))
    (pad 8 smd rect (at 2.87 1.95 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 75 /+3.3V))
    (pad 9 smd rect (at 2.87 1.3 180) (size 1.57 0.41) (layers Front F.Paste F.Mask))
    (pad 10 smd rect (at 2.87 0.65 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 74 GND))
    (pad 11 smd rect (at 2.87 0 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 8 /BFPRST))
    (pad 12 smd rect (at 2.87 -0.65 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 9 /BFPDO))
    (pad 13 smd rect (at 2.87 -1.3 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 12 /BFPDI))
    (pad 14 smd rect (at 2.87 -1.95 180) (size 1.57 0.41) (layers Front F.Paste F.Mask)
      (net 76 /+5V))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 127.9525 84.709 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R6 (at 3.683 0 180) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 76 /+5V))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 8 /BFPRST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 148.9075 78.235 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R5 (at -3.051 0.0635 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 /RST))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 131.953 84.706 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R2 (at 3.6165 0 180) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 76 /+5V))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 9 /BFPDO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 151.384 82.6165 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R3 (at -3.2355 -0.0635 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 22 /RXD))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 135.128 84.706 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R4 (at 3.553 -0.127 180) (layer F.SilkS))
    (fp_text value 1k5 (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 76 /+5V))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 12 /BFPDI))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 154.3685 83.95 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R1 (at -3.172 -0.0635 180) (layer F.SilkS))
    (fp_text value 1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 35 /TXD))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 154.3685 78.229 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C8 (at -3.045 0.127 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_JST:JST_PH_S12B-PH-K_1x12_P2.00mm_Horizontal (layer Front) (tedit 5B7745C6)
    (at 119.9515 89.662)
    (descr "JST PH series connector, S12B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
    (tags "connector JST PH top entry")
    (fp_text reference J1 (at 11 -2.55) (layer F.SilkS))
    (fp_text value Conn_01x12 (at 11 7.45) (layer F.Fab))
    (fp_text user %R (at 11 2.5) (layer F.Fab))
    (pad 12 thru_hole oval (at 22 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 11 thru_hole oval (at 20 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 12 /BFPDI))
    (pad 10 thru_hole oval (at 18 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 11 /+18V_FLT))
    (pad 9 thru_hole oval (at 16 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 8 thru_hole oval (at 14 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 10 /FIL2))
    (pad 7 thru_hole oval (at 12 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 9 /BFPDO))
    (pad 6 thru_hole oval (at 10 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 1 /-18V_FP))
    (pad 5 thru_hole oval (at 8 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 8 /BFPRST))
    (pad 4 thru_hole oval (at 6 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 3 thru_hole oval (at 4 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 7 /FPSTBY))
    (pad 2 thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask)
      (net 6 /FIL1))
    (pad 1 thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333)
      (net 5 /FPREF))
    (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S12B-PH-K_1x12_P2.00mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 216.662 89.027)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R22 (at -3.683 -1.016) (layer F.SilkS))
    (fp_text value 22 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 67 "Net-(J4-Pad6)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 73 /SWO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 216.665 86.487)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R21 (at -3.6225 -0.889) (layer F.SilkS))
    (fp_text value 22 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 68 "Net-(J4-Pad5)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 66 /NRST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 216.659 83.947)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R20 (at -3.68 -0.635) (layer F.SilkS))
    (fp_text value 22 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 69 "Net-(J4-Pad4)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 72 /SWDIO))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 216.662 78.867)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R19 (at -3.8735 -0.4445) (layer F.SilkS))
    (fp_text value 22 (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 70 "Net-(J4-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 71 /SWCLK))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Horizontal (layer Front) (tedit 59FED5CB)
    (at 222.3135 76.327)
    (descr "Through hole angled pin header, 1x06, 2.54mm pitch, 6mm pin length, single row")
    (tags "Through hole angled pin header THT 1x06 2.54mm single row")
    (fp_text reference J4 (at 2.032 -2.9845) (layer F.SilkS))
    (fp_text value SWD (at 2.032 15.621) (layer F.SilkS))
    (fp_text user %R (at 2.77 6.35 90) (layer F.Fab))
    (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 67 "Net-(J4-Pad6)"))
    (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 68 "Net-(J4-Pad5)"))
    (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 69 "Net-(J4-Pad4)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 70 "Net-(J4-Pad2)"))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Horizontal.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Crystal:Crystal_SMD_Abracon_ABM3B-4Pin_5.0x3.2mm (layer Front) (tedit 5A0FD1B2)
    (at 175.768 98.4885)
    (descr "Abracon Miniature Ceramic Smd Crystal ABM3B http://www.abracon.com/Resonators/abm3b.pdf, 5.0x3.2mm^2 package")
    (tags "SMD SMT crystal")
    (attr smd)
    (fp_text reference Y1 (at 0 -2.8) (layer F.SilkS))
    (fp_text value 16MHz (at 0 2.8) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 4 smd rect (at -2 -1.2) (size 1.8 1.2) (layers Front F.Paste F.Mask)
      (net 74 GND))
    (pad 3 smd rect (at 2 -1.2) (size 1.8 1.2) (layers Front F.Paste F.Mask)
      (net 62 "Net-(C15-Pad1)"))
    (pad 2 smd rect (at 2 1.2) (size 1.8 1.2) (layers Front F.Paste F.Mask)
      (net 74 GND))
    (pad 1 smd rect (at -2 1.2) (size 1.8 1.2) (layers Front F.Paste F.Mask)
      (net 61 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Crystal.3dshapes/Crystal_SMD_Abracon_ABM3B-4Pin_5.0x3.2mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 224.5 107.2)
    (fp_text reference SW18 (at -0.0275 -4.3935) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 28 /KP_R0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 32 /KP_C4) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 236 107.2)
    (fp_text reference SW17 (at 0 -4.3935) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 27 /KP_R1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 32 /KP_C4) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 197 120.95)
    (fp_text reference SW15 (at -0.023 -4.237) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 27 /KP_R1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 31 /KP_C3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 197 132.7)
    (fp_text reference SW14 (at -0.023 -4.2395) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 26 /KP_R2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 31 /KP_C3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 76.5 109.2)
    (fp_text reference SW13 (at 0 -4.171) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 24 /KP_R3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 31 /KP_C3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 106 132.7)
    (fp_text reference SW12 (at -0.0185 -4.1125) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 28 /KP_R0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 30 /KP_C2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 134.5 132.7)
    (fp_text reference SW11 (at -0.007 -4.2395) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 27 /KP_R1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 30 /KP_C2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 151.5 132.7)
    (fp_text reference SW10 (at 0 -4.2395) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 26 /KP_R2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 30 /KP_C2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 180 132.7)
    (fp_text reference SW9 (at 0 -4.2395) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 24 /KP_R3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 30 /KP_C2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 106 120.95)
    (fp_text reference SW8 (at -0.0185 -4.1735) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 28 /KP_R0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 29 /KP_C1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 134.5 120.95)
    (fp_text reference SW7 (at -0.007 -4.11) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 27 /KP_R1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 29 /KP_C1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 151.5 120.95)
    (fp_text reference SW6 (at 0 -4.0465) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 26 /KP_R2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 29 /KP_C1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 180 120.95)
    (fp_text reference SW5 (at 0 -4.1735) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 24 /KP_R3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 29 /KP_C1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 106 109.2)
    (fp_text reference SW4 (at -0.0185 -4.2345) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 28 /KP_R0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 25 /KP_C0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 134.5 109.2)
    (fp_text reference SW3 (at -0.007 -4.171) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 27 /KP_R1) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 25 /KP_C0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 151.5 109.2)
    (fp_text reference SW2 (at 0 -4.1075) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 26 /KP_R2) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 25 /KP_C0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 180 109.2)
    (fp_text reference SW1 (at 0 -4.1075) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 24 /KP_R3) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 25 /KP_C0) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module hp34970:contact2 (layer Front) (tedit 5F668F76)
    (at 76.5 127.7)
    (fp_text reference SW20 (at -0.046 -4.383) (layer F.SilkS))
    (fp_text value SW_Push_45deg (at 0 3.375) (layer F.Fab))
    (pad 2 smd custom (at 0 -0.2 180) (size 0.18 0.18) (layers Front F.Mask)
      (net 74 GND) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
    (pad 1 smd custom (at 0 0.2) (size 0.18 0.18) (layers Front F.Mask)
      (net 7 /FPSTBY) (zone_connect 0)
      (options (clearance outline) (anchor circle))
      (primitives
        (gr_arc (start 0 -0.2) (end 0 2.4) (angle 147.8) (width 0.2))
        (gr_line (start 0.6 2.4) (end 0 2.4) (width 0.18))
        (gr_line (start 1.265 1.6) (end -1.8762 1.6) (width 0.18))
        (gr_line (start 1.9596 0.8) (end -2.4 0.8) (width 0.18))
        (gr_line (start 2.1879 0) (end -2.5923 0) (width 0.18))
        (gr_line (start 2.1166 -0.8) (end -2.5298 -0.8) (width 0.18))
        (gr_line (start 1.6497 -1.6) (end -2.1909 -1.6) (width 0.18))
        (gr_line (start 0.2471 -2.4) (end -1.3856 -2.4) (width 0.18))
      ))
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 192.659 78.356 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C16 (at -3.175 0.0635 180) (layer F.SilkS))
    (fp_text value 10u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at -0.13 -1.905 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer Front) (tedit 5A02FE31)
    (at 76.6064 87.2998 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW22 (at 9.1694 2.2098 90) (layer F.SilkS))
    (fp_text value DFU (at 3.75 6.7) (layer F.SilkS))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(R18-Pad1)"))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 /+3.3V))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 65 "Net-(R18-Pad1)"))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Button_Switch_THT:SW_PUSH_6mm_H5mm (layer Front) (tedit 5A02FE31)
    (at 76.6064 77.216 180)
    (descr "tactile push button, 6x6mm e.g. PHAP33xx series, height=5mm")
    (tags "tact sw push 6mm")
    (fp_text reference SW21 (at 9.1694 2.286 90) (layer F.SilkS))
    (fp_text value RESET (at 3.75 6.7) (layer F.SilkS))
    (fp_text user %R (at 3.25 2.25) (layer F.Fab))
    (pad 1 thru_hole circle (at 6.5 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 2 thru_hole circle (at 6.5 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 /NRST))
    (pad 1 thru_hole circle (at 0 0 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 2 thru_hole circle (at 0 4.5 270) (size 2 2) (drill 1.1) (layers *.Cu *.Mask)
      (net 66 /NRST))
    (model ${KISYS3DMOD}/Button_Switch_THT.3dshapes/SW_PUSH_6mm_H5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 82.293 87.3125)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R18 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 65 "Net-(R18-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 173.5328 79.3018 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R17 (at -3.1653 -0.1397 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 66 /NRST))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 171.1325 82.1085 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C17 (at 3.1399 -0.5842 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 66 /NRST))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 104.013 87.3409 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C13 (at 4.2261 0.0635 90) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 /+18V_FLT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 180.594 98.552 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C15 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 18p (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 62 "Net-(C15-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 170.942 98.549 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C14 (at 0.0605 -2.794 180) (layer F.SilkS))
    (fp_text value 18p (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 61 "Net-(C14-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "hp34970:Bourns SNR2050TA inductor" (layer Front) (tedit 5F5AAB12)
    (at 107.4039 81.1276 90)
    (fp_text reference L1 (at 3.3401 0.1651 180) (layer F.SilkS))
    (fp_text value 8.2uH (at 0 -0.5 90) (layer F.Fab))
    (pad 2 smd rect (at 1.8 0 90) (size 1.5 4.7) (layers Front F.Paste F.Mask)
      (net 76 /+5V))
    (pad 1 smd rect (at -1.8 0 90) (size 1.5 4.7) (layers Front F.Paste F.Mask)
      (net 4 "Net-(C9-Pad1)"))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 96.9264 81.0671 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R16 (at 1.3746 -2.5019 180) (layer F.SilkS))
    (fp_text value 294k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 60 "Net-(IC1-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hp34970:MOLEX_500075-1517 (layer Front) (tedit 5F5A999C)
    (at 82.6516 79.5706 270)
    (fp_text reference J2 (at -0.825 -4.135 90) (layer F.SilkS))
    (fp_text value USB_B (at 6.795 4.135 90) (layer F.Fab))
    (pad 1 thru_hole circle (at -1.6 1.3 270) (size 1.15 1.15) (drill 0.75) (layers *.Cu *.Mask)
      (net 14 "Net-(J2-Pad1)"))
    (pad 2 thru_hole circle (at -0.8 -1.3 270) (size 1.15 1.15) (drill 0.75) (layers *.Cu *.Mask)
      (net 13 /D-))
    (pad 3 thru_hole circle (at 0 1.3 270) (size 1.15 1.15) (drill 0.75) (layers *.Cu *.Mask)
      (net 15 /D+))
    (pad 4 thru_hole circle (at 0.8 -1.3 270) (size 1.15 1.15) (drill 0.75) (layers *.Cu *.Mask)
      (net 59 "Net-(J2-Pad4)"))
    (pad 5 thru_hole circle (at 1.6 1.3 270) (size 1.15 1.15) (drill 0.75) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad S1 thru_hole oval (at -3.65 0 270) (size 2 4) (drill oval 0.7 2.45) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad S2 thru_hole oval (at 3.65 0 270) (size 2 4) (drill oval 0.7 2.45) (layers *.Cu *.Mask)
      (net 74 GND))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 87.5284 83.5884 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R15 (at 1.4829 2.9591 180) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 59 "Net-(J2-Pad4)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module hp34970:bourns_ECW0J-C24-EE24L (layer Front) (tedit 5F5ABB1F)
    (at 214 127.7 270)
    (fp_text reference SW19 (at 2.475 4.196 180) (layer F.SilkS))
    (fp_text value Rotary_Encoder (at 0 -0.5 90) (layer F.Fab))
    (pad "" np_thru_hole circle (at 11.4 -23.6 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.4 -23.6 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -11.4 -8.4 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 11.4 -8.4 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask))
    (pad B thru_hole circle (at 2.54 0 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask)
      (net 34 /RE_B))
    (pad C thru_hole circle (at 0 0 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask)
      (net 75 /+3.3V))
    (pad A thru_hole rect (at -2.54 0 270) (size 1.524 1.524) (drill 1.2) (layers *.Cu *.Mask)
      (net 33 /RE_A))
  )
  (module hp34970:SSD1322_DSP locked (layer Front) (tedit 5F5CB927)
    (at 204.00264 93.25356)
    (fp_text reference J3 (at 0.3 0.3) (layer F.SilkS))
    (fp_text value Conn_02x08_Odd_Even (at 0.3 -0.7) (layer F.Fab))
    (pad "" np_thru_hole circle (at -93.94952 -22.90064 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at -93.94952 5.59816 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.05156 5.60324 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad "" np_thru_hole circle (at 1.05156 -22.90064 180) (size 3 3) (drill 3) (layers *.Cu *.Mask))
    (pad 16 thru_hole circle (at 2.54 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 16 /DSP_CS))
    (pad 15 thru_hole circle (at 0 -17.78 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 77 /~DSP_RST))
    (pad 14 thru_hole circle (at 2.54 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 17 /DSP_DC))
    (pad 13 thru_hole circle (at 0 -15.24 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 12 thru_hole circle (at 2.54 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 11 thru_hole circle (at 0 -12.7 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 10 thru_hole circle (at 2.54 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 9 thru_hole circle (at 0 -10.16 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 8 thru_hole circle (at 2.54 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 7 thru_hole circle (at 0 -7.62 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
    (pad 6 thru_hole circle (at 2.54 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 18 "Net-(J3-Pad6)"))
    (pad 5 thru_hole circle (at 0 -5.08 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 19 /DSP_DI))
    (pad 4 thru_hole circle (at 2.54 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 20 /DSP_SCLK))
    (pad 3 thru_hole circle (at 0 -2.54 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 21 "Net-(J3-Pad3)"))
    (pad 2 thru_hole circle (at 2.54 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 76 /+5V))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 74 GND))
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 99.568 84.8106 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R14 (at 4.1559 -0.0254) (layer F.SilkS))
    (fp_text value 750k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 60 "Net-(IC1-Pad4)"))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 /+18V_FLT))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_TO_SOT_SMD:SOT-23-6 (layer Front) (tedit 5A02FF57)
    (at 100.0379 81.1276 270)
    (descr "6-pin SOT-23 package")
    (tags SOT-23-6)
    (attr smd)
    (fp_text reference IC1 (at -2.7051 -0.2286 180) (layer F.SilkS))
    (fp_text value TPS560430YFDBV (at 0 2.9 90) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 5 smd rect (at 1.1 0 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 11 /+18V_FLT))
    (pad 6 smd rect (at 1.1 -0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 4 "Net-(C9-Pad1)"))
    (pad 4 smd rect (at 1.1 0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 60 "Net-(IC1-Pad4)"))
    (pad 3 smd rect (at -1.1 0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad3)"))
    (pad 2 smd rect (at -1.1 0 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 74 GND))
    (pad 1 smd rect (at -1.1 -0.95 270) (size 1.06 0.65) (layers Front F.Paste F.Mask)
      (net 3 "Net-(C9-Pad2)"))
    (model ${KISYS3DMOD}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_QFP:LQFP-64_10x10mm_P0.5mm (layer Front) (tedit 5D9F72AF)
    (at 182.9435 88.8365 90)
    (descr "LQFP, 64 Pin (https://www.analog.com/media/en/technical-documentation/data-sheets/ad7606_7606-6_7606-4.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
    (tags "LQFP QFP")
    (attr smd)
    (fp_text reference U2 (at 6.223 5.3975 180) (layer F.SilkS))
    (fp_text value STM32F303RDTx (at 0 7.4 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 64 smd roundrect (at -3.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /+3.3V))
    (pad 63 smd roundrect (at -3.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 GND))
    (pad 62 smd roundrect (at -2.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 36 "Net-(U2-Pad62)"))
    (pad 61 smd roundrect (at -2.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 24 /KP_R3))
    (pad 60 smd roundrect (at -1.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 65 "Net-(R18-Pad1)"))
    (pad 59 smd roundrect (at -1.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 26 /KP_R2))
    (pad 58 smd roundrect (at -0.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 27 /KP_R1))
    (pad 57 smd roundrect (at -0.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 28 /KP_R0))
    (pad 56 smd roundrect (at 0.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 31 /KP_C3))
    (pad 55 smd roundrect (at 0.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 73 /SWO))
    (pad 54 smd roundrect (at 1.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 37 "Net-(U2-Pad54)"))
    (pad 53 smd roundrect (at 1.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 38 "Net-(U2-Pad53)"))
    (pad 52 smd roundrect (at 2.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 39 "Net-(U2-Pad52)"))
    (pad 51 smd roundrect (at 2.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 40 "Net-(U2-Pad51)"))
    (pad 50 smd roundrect (at 3.25 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 2 /RST))
    (pad 49 smd roundrect (at 3.75 -5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 71 /SWCLK))
    (pad 48 smd roundrect (at 5.675 -3.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /+3.3V))
    (pad 47 smd roundrect (at 5.675 -3.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 GND))
    (pad 46 smd roundrect (at 5.675 -2.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 72 /SWDIO))
    (pad 45 smd roundrect (at 5.675 -2.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 15 /D+))
    (pad 44 smd roundrect (at 5.675 -1.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 13 /D-))
    (pad 43 smd roundrect (at 5.675 -1.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 41 "Net-(U2-Pad43)"))
    (pad 42 smd roundrect (at 5.675 -0.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 42 "Net-(U2-Pad42)"))
    (pad 41 smd roundrect (at 5.675 -0.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 43 "Net-(U2-Pad41)"))
    (pad 40 smd roundrect (at 5.675 0.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 44 "Net-(U2-Pad40)"))
    (pad 39 smd roundrect (at 5.675 0.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 45 "Net-(U2-Pad39)"))
    (pad 38 smd roundrect (at 5.675 1.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 46 "Net-(U2-Pad38)"))
    (pad 37 smd roundrect (at 5.675 1.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 47 "Net-(U2-Pad37)"))
    (pad 36 smd roundrect (at 5.675 2.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 48 "Net-(U2-Pad36)"))
    (pad 35 smd roundrect (at 5.675 2.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 49 "Net-(U2-Pad35)"))
    (pad 34 smd roundrect (at 5.675 3.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 50 "Net-(U2-Pad34)"))
    (pad 33 smd roundrect (at 5.675 3.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 51 "Net-(U2-Pad33)"))
    (pad 32 smd roundrect (at 3.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /+3.3V))
    (pad 31 smd roundrect (at 3.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 GND))
    (pad 30 smd roundrect (at 2.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 52 "Net-(U2-Pad30)"))
    (pad 29 smd roundrect (at 2.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 53 "Net-(U2-Pad29)"))
    (pad 28 smd roundrect (at 1.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 63 "Net-(U2-Pad28)"))
    (pad 27 smd roundrect (at 1.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 64 "Net-(U2-Pad27)"))
    (pad 26 smd roundrect (at 0.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 32 /KP_C4))
    (pad 25 smd roundrect (at 0.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 22 /RXD))
    (pad 24 smd roundrect (at -0.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 35 /TXD))
    (pad 23 smd roundrect (at -0.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 19 /DSP_DI))
    (pad 22 smd roundrect (at -1.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 54 /MISO))
    (pad 21 smd roundrect (at -1.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 20 /DSP_SCLK))
    (pad 20 smd roundrect (at -2.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 17 /DSP_DC))
    (pad 19 smd roundrect (at -2.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /+3.3V))
    (pad 18 smd roundrect (at -3.25 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 GND))
    (pad 17 smd roundrect (at -3.75 5.675 90) (size 0.3 1.55) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 77 /~DSP_RST))
    (pad 16 smd roundrect (at -5.675 3.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 16 /DSP_CS))
    (pad 15 smd roundrect (at -5.675 3.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 33 /RE_A))
    (pad 14 smd roundrect (at -5.675 2.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 34 /RE_B))
    (pad 13 smd roundrect (at -5.675 2.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /+3.3V))
    (pad 12 smd roundrect (at -5.675 1.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 74 GND))
    (pad 11 smd roundrect (at -5.675 1.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 55 "Net-(U2-Pad11)"))
    (pad 10 smd roundrect (at -5.675 0.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 25 /KP_C0))
    (pad 9 smd roundrect (at -5.675 0.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 29 /KP_C1))
    (pad 8 smd roundrect (at -5.675 -0.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 30 /KP_C2))
    (pad 7 smd roundrect (at -5.675 -0.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 66 /NRST))
    (pad 6 smd roundrect (at -5.675 -1.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 62 "Net-(C15-Pad1)"))
    (pad 5 smd roundrect (at -5.675 -1.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 61 "Net-(C14-Pad1)"))
    (pad 4 smd roundrect (at -5.675 -2.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 56 "Net-(U2-Pad4)"))
    (pad 3 smd roundrect (at -5.675 -2.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 57 "Net-(U2-Pad3)"))
    (pad 2 smd roundrect (at -5.675 -3.25 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 58 "Net-(U2-Pad2)"))
    (pad 1 smd roundrect (at -5.675 -3.75 90) (size 1.55 0.3) (layers Front F.Paste F.Mask) (roundrect_rratio 0.25)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Package_QFP.3dshapes/LQFP-64_10x10mm_P0.5mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 95.6945 75.943 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R12 (at 3.045 2.667 180) (layer F.SilkS))
    (fp_text value 22.1k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0.1016 -0.0254 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(IC1-Pad3)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 98.171 75.949 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R11 (at -3.051 2.7305 180) (layer F.SilkS))
    (fp_text value 88.7k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0.1494 0.0889 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 23 "Net-(IC1-Pad3)"))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 76 /+5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric (layer Front) (tedit 5B301BBD)
    (at 177.67 77.978)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags resistor)
    (attr smd)
    (fp_text reference R10 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 1.5k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 15 /D+))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 112.9538 80.7496 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C11 (at -3.1526 -0.0127 180) (layer F.SilkS))
    (fp_text value 15u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 76 /+5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 106.5022 87.3476 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C10 (at 4.2829 0.0762 90) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 11 /+18V_FLT))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 103.3399 81.1306 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C9 (at 3.0891 -0.1524 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 3 "Net-(C9-Pad2)"))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 4 "Net-(C9-Pad1)"))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 185.6008 97.155 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C7 (at -3.5022 0.127) (layer F.SilkS))
    (fp_text value 10n (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 185.6008 99.695 180)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C6 (at -3.5022 0) (layer F.SilkS))
    (fp_text value 1u (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 180) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 180) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 177.67 80.645)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C5 (at 3.432 0) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 174.371 93.5004 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C4 (at 3.0129 -0.0635 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 191.135 85.341 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C3 (at -1.4575 -2.3495 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 191.135 93.4115 270)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C2 (at 1.521 -2.0955 180) (layer F.SilkS))
    (fp_text value 100n (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 270) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer Front) (tedit 5B301BBE)
    (at 172.085 93.4974 90)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at -1.4986 -2.032 180) (layer F.SilkS))
    (fp_text value 4.7u (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 74 GND))
    (pad 1 smd roundrect (at -1.4 0 90) (size 1.25 1.75) (layers Front F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 75 /+3.3V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_text DFU (at 73.4568 85.1916) (layer B.SilkS))
  (gr_text RESET (at 73.406 74.8792) (layer B.SilkS))
  (gr_text "To force DFU mode, press the DFU button while powering up/reset" (at 88.6968 67.1576) (layer B.SilkS))
  (gr_text "SSD1322 OLED 256x64" (at 200.5076 83.9724 90) (layer F.SilkS))
  (gr_text "HP34970 Replacement Front Panel" (at 99.4664 122.7836) (layer B.SilkS))
  (gr_text "REG. 3.3V" (at 188.595 69.9135) (layer F.SilkS))
  (gr_text "REG. 5V" (at 103.4415 74.9935) (layer F.SilkS))
  (dimension 5.5 (width 0.1524) (layer Dwgs.User)
    (gr_text "5.500 mm" (at 100.225 55.575201) (layer Dwgs.User))
    (feature1 (pts (xy 102.975 61.411501) (xy 102.975 56.30958)))
    (feature2 (pts (xy 97.475 61.411501) (xy 97.475 56.30958)))
    (crossbar (pts (xy 97.475 56.896001) (xy 102.975 56.896001)))
    (arrow1a (pts (xy 102.975 56.896001) (xy 101.848496 57.482422)))
    (arrow1b (pts (xy 102.975 56.896001) (xy 101.848496 56.30958)))
    (arrow2a (pts (xy 97.475 56.896001) (xy 98.601504 57.482422)))
    (arrow2b (pts (xy 97.475 56.896001) (xy 98.601504 56.30958)))
  )
  (dimension 31 (width 0.1524) (layer Dwgs.User)
    (gr_text "31.000 mm" (at 229.975 55.5752) (layer Dwgs.User))
    (feature1 (pts (xy 245.475 61.4115) (xy 245.475 56.309579)))
    (feature2 (pts (xy 214.475 61.4115) (xy 214.475 56.309579)))
    (crossbar (pts (xy 214.475 56.896) (xy 245.475 56.896)))
    (arrow1a (pts (xy 245.475 56.896) (xy 244.348496 57.482421)))
    (arrow1b (pts (xy 245.475 56.896) (xy 244.348496 56.309579)))
    (arrow2a (pts (xy 214.475 56.896) (xy 215.601504 57.482421)))
    (arrow2b (pts (xy 214.475 56.896) (xy 215.601504 56.309579)))
  )
  (dimension 34 (width 0.1524) (layer Dwgs.User)
    (gr_text "34.000 mm" (at 80.475 55.575201) (layer Dwgs.User))
    (feature1 (pts (xy 97.475 62.4115) (xy 97.475 56.30958)))
    (feature2 (pts (xy 63.475 62.4115) (xy 63.475 56.30958)))
    (crossbar (pts (xy 63.475 56.896001) (xy 97.475 56.896001)))
    (arrow1a (pts (xy 97.475 56.896001) (xy 96.348496 57.482422)))
    (arrow1b (pts (xy 97.475 56.896001) (xy 96.348496 56.30958)))
    (arrow2a (pts (xy 63.475 56.896001) (xy 64.601504 57.482422)))
    (arrow2b (pts (xy 63.475 56.896001) (xy 64.601504 56.30958)))
  )
  (dimension 78.3 (width 0.1524) (layer Dwgs.User)
    (gr_text "78.300 mm" (at 58.3692 100.5615 270) (layer Dwgs.User))
    (feature1 (pts (xy 64.475 139.7115) (xy 59.103579 139.7115)))
    (feature2 (pts (xy 64.475 61.4115) (xy 59.103579 61.4115)))
    (crossbar (pts (xy 59.69 61.4115) (xy 59.69 139.7115)))
    (arrow1a (pts (xy 59.69 139.7115) (xy 59.103579 138.584996)))
    (arrow1b (pts (xy 59.69 139.7115) (xy 60.276421 138.584996)))
    (arrow2a (pts (xy 59.69 61.4115) (xy 59.103579 62.538004)))
    (arrow2b (pts (xy 59.69 61.4115) (xy 60.276421 62.538004)))
  )
  (dimension 182 (width 0.1524) (layer Dwgs.User)
    (gr_text "182.000 mm" (at 154.475 52.0192) (layer Dwgs.User))
    (feature1 (pts (xy 245.475 62.4115) (xy 245.475 52.753579)))
    (feature2 (pts (xy 63.475 62.4115) (xy 63.475 52.753579)))
    (crossbar (pts (xy 63.475 53.34) (xy 245.475 53.34)))
    (arrow1a (pts (xy 245.475 53.34) (xy 244.348496 53.926421)))
    (arrow1b (pts (xy 245.475 53.34) (xy 244.348496 52.753579)))
    (arrow2a (pts (xy 63.475 53.34) (xy 64.601504 53.926421)))
    (arrow2b (pts (xy 63.475 53.34) (xy 64.601504 52.753579)))
  )
  (dimension 79.5 (width 0.1524) (layer Dwgs.User)
    (gr_text "79.500 mm" (at 252.6538 101.1615 270) (layer Dwgs.User))
    (feature1 (pts (xy 244.475 140.9115) (xy 251.919421 140.9115)))
    (feature2 (pts (xy 244.475 61.4115) (xy 251.919421 61.4115)))
    (crossbar (pts (xy 251.333 61.4115) (xy 251.333 140.9115)))
    (arrow1a (pts (xy 251.333 140.9115) (xy 250.746579 139.784996)))
    (arrow1b (pts (xy 251.333 140.9115) (xy 251.919421 139.784996)))
    (arrow2a (pts (xy 251.333 61.4115) (xy 250.746579 62.538004)))
    (arrow2b (pts (xy 251.333 61.4115) (xy 251.919421 62.538004)))
  )
  (dimension 111.5 (width 0.1524) (layer Dwgs.User)
    (gr_text "111.500 mm" (at 158.725 55.5752 5.138634934e-07) (layer Dwgs.User))
    (feature1 (pts (xy 214.475 61.4115) (xy 214.475 56.309579)))
    (feature2 (pts (xy 102.975 61.411501) (xy 102.975 56.30958)))
    (crossbar (pts (xy 102.975 56.896001) (xy 214.475 56.896)))
    (arrow1a (pts (xy 214.475 56.896) (xy 213.348496 57.482421)))
    (arrow1b (pts (xy 214.475 56.896) (xy 213.348496 56.309579)))
    (arrow2a (pts (xy 102.975 56.896001) (xy 104.101504 57.482422)))
    (arrow2b (pts (xy 102.975 56.896001) (xy 104.101504 56.30958)))
  )
  (dimension 93.317027 (width 0.1524) (layer Cmts.User)
    (gr_text "93.317 mm" (at 167.822806 53.029965 -0.04328634319) (layer Cmts.User))
    (feature1 (pts (xy 121.158 61.341) (xy 121.163751 53.729094)))
    (feature2 (pts (xy 214.475 61.4115) (xy 214.480751 53.799594)))
    (crossbar (pts (xy 214.480308 54.386015) (xy 121.163308 54.315515)))
    (arrow1a (pts (xy 121.163308 54.315515) (xy 122.290254 53.729945)))
    (arrow1b (pts (xy 121.163308 54.315515) (xy 122.289368 54.902787)))
    (arrow2a (pts (xy 214.480308 54.386015) (xy 213.354248 53.798743)))
    (arrow2b (pts (xy 214.480308 54.386015) (xy 213.353362 54.971585)))
  )
  (dimension 111.5 (width 0.1524) (layer Cmts.User)
    (gr_text "111.500 mm" (at 158.725 62.7323 5.138634934e-07) (layer Cmts.User))
    (feature1 (pts (xy 214.475 61.4115) (xy 214.475 61.997921)))
    (feature2 (pts (xy 102.975 61.411501) (xy 102.975 61.997922)))
    (crossbar (pts (xy 102.975 61.411501) (xy 214.475 61.4115)))
    (arrow1a (pts (xy 214.475 61.4115) (xy 213.348496 61.997921)))
    (arrow1b (pts (xy 214.475 61.4115) (xy 213.348496 60.825079)))
    (arrow2a (pts (xy 102.975 61.411501) (xy 104.101504 61.997922)))
    (arrow2b (pts (xy 102.975 61.411501) (xy 104.101504 60.82508)))
  )
  (gr_text "CC-BY-SA - David Douard\nhttps://whatever.sdfa3.org/tag/34970a.html" (at 103.0605 126.873) (layer B.SilkS))
  (gr_text JLCJLCJLCJLC (at 125.095 93.9165) (layer F.SilkS))
  (gr_text GND_FLT (at 141.9225 87.9475 270) (layer B.SilkS))
  (gr_text BFPDI (at 139.954 87.9475 270) (layer B.SilkS))
  (gr_text +18V_FP (at 137.795 87.9475 270) (layer B.SilkS))
  (gr_text GND_FLT (at 135.89 87.9475 270) (layer B.SilkS))
  (gr_text "FIL2 (NC)" (at 133.985 87.9475 270) (layer B.SilkS))
  (gr_text BFPDO (at 131.953 87.9475 270) (layer B.SilkS))
  (gr_text "-18V_FP (NC)" (at 129.9845 87.9475 270) (layer B.SilkS))
  (gr_text BFPRST (at 127.9525 87.9475 270) (layer B.SilkS))
  (gr_text GND_FLT (at 125.984 87.9475 270) (layer B.SilkS))
  (gr_text FP_STBY (at 123.952 87.9475 270) (layer B.SilkS))
  (gr_text "FIL1 (NC)" (at 121.92 87.9475 270) (layer B.SilkS))
  (gr_text "FPREF (NC)" (at 120.015 87.9475 270) (layer B.SilkS))
  (gr_text SWO (at 234.442 89.027) (layer F.SilkS))
  (gr_text NRST (at 234.442 86.487) (layer F.SilkS))
  (gr_text SWDIO (at 234.5055 83.947) (layer F.SilkS))
  (gr_text GND (at 234.5055 81.407) (layer F.SilkS))
  (gr_text SWCLK (at 234.3785 78.9305) (layer F.SilkS))
  (gr_text VDD (at 234.2515 76.2635) (layer F.SilkS))
  (gr_line (start 245.475 139.9115) (end 245.475 105.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.075 68.411501) (end 141.075 68.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 223.475 142.4115) (end 213.475 142.4115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.475 140.7115) (end 213.475 142.4115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 244.475 61.4115) (end 214.475 61.4115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 101.975 64.7115) (end 98.475 64.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.475 61.411501) (end 64.475 61.4115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 124.474999 140.711501) (end 124.474999 139.711501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 101.975 63.7115) (end 101.975 64.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.275 61.411501) (end 142.275 66.011501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 158.275 67.211501) (end 158.275 67.211501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.975 139.711501) (end 64.475 139.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.475 139.711501) (end 124.474999 139.711501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 93.975 134.711501) (end 95.075 134.711501) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 119.474999 97.411501) (end 119.474999 96.411501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 244.475 94.4115) (end 244.475 93.4115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 213.475 64.7115) (end 209.975 64.7115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 169.575 135.711501) (end 170.575 135.711501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.875 61.411501) (end 102.975 61.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 245.475 93.4115) (end 245.475 62.4115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 119.474999 96.411501) (end 142.475 96.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 102.975 61.411501) (end 102.975 63.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 245.475 105.7115) (end 244.475 105.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 243.475 104.7115) (end 243.475 94.4115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 119.474999 101.411501) (end 118.474999 101.411501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 244.475 62.4115) (end 245.475 62.4115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.475 93.4115) (end 63.475 93.4115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 93.975 135.711501) (end 93.975 134.711501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.475 105.7115) (end 63.475 138.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 65.475 94.4115) (end 65.475 104.7115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 244.475 139.9115) (end 244.475 140.9115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 170.575 135.711501) (end 170.575 139.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 208.975 61.4115) (end 142.275 61.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 224.475 140.9115) (end 244.475 140.9115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 167.475 135.711501) (end 167.475 139.711501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 97.475 61.411501) (end 97.475 63.7115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 157.075 67.211501) (end 157.075 68.411501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 64.475 94.4115) (end 65.475 94.4115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 245.475 93.4115) (end 244.475 93.4115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 168.475 135.711501) (end 168.475 134.711501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 95.075 135.711501) (end 96.075 135.711501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 143.475 97.411501) (end 143.475 101.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.475 142.411501) (end 114.475 142.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 92.975 135.711501) (end 92.975 139.711501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 168.475 134.711501) (end 169.575 134.711501) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 64.474999 138.7115) (end 63.475 138.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 64.475 105.7115) (end 63.475 105.7115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 209.975 63.7115) (end 208.975 63.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 157.075 67.211501) (end 158.275 67.211501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 223.475 141.9115) (end 223.475 142.4115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 214.475 63.7115) (end 214.475 61.4115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 224.475 141.9115) (end 224.475 140.9115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 64.474999 62.4115) (end 64.475 61.4115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 114.475 140.711501) (end 114.475 142.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 212.475 139.7115) (end 170.575 139.7115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 118.474999 101.411501) (end 118.474999 97.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 123.475 140.711501) (end 123.475 142.411501) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 142.475 97.411501) (end 143.475 97.411501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 113.475 139.711501) (end 96.075 139.711501) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 213.475 63.7115) (end 213.475 64.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 98.475 63.7115) (end 97.475 63.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 139.875 61.411501) (end 139.875 67.211501) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 141.075 67.211501) (end 139.875 67.211501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 208.975 63.7115) (end 208.975 61.4115) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 113.475 140.711501) (end 114.475 140.711501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 96.075 135.711501) (end 96.075 139.711501) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 64.475 104.7115) (end 64.474999 105.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 142.475 101.411501) (end 142.475 102.411501) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 212.475 140.7115) (end 213.475 140.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 142.475 102.411501) (end 119.474999 102.411501) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 63.475 62.4115) (end 63.475 93.4115) (layer Edge.Cuts) (width 0.05))
  (gr_line (start 157.075 66.011501) (end 142.275 66.011501) (layer Edge.Cuts) (width 0.05))
  (gr_arc (start 244.475 104.7115) (end 243.475 104.7115) (angle -90) (layer Edge.Cuts) (width 0.05))
  (zone (net 74) (net_name GND) (layer Front) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 243.9416 138.6332) (xy 64.5668 138.6332) (xy 64.5668 62.5348) (xy 243.9416 62.5348)
      )
    )
  )
  (zone (net 74) (net_name GND) (layer Back) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 32) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 243.933222 138.6332) (xy 64.558422 138.6332) (xy 64.558422 62.5348) (xy 243.933222 62.5348)
      )
    )
  )
)
