========================================
 EIP 545B RF Frequency Counter - Part 2
========================================

:author: David Douard
:Category: Electronics
:Tags: test equipment, RF, EIP, 545B, counter
:series: EIP545B Frequency Counter
:series_index: 2

I've started a discussion_ on the `eevblog forum`_ to gather a bit help for my
project. And I did well since a few fellows did help me a lot on some aspects.

I have now been able to run the power meter at full resolution (even if it's
very out of calibration), and have been able to locate where these annoying
default settings are set (tip: unfortunately not in the EEPROM, but in the
firmware).

I've also digged a bit more for the sensitivity problem on band 3. I still
haven't foudn yet the true culprit, but now I have a few tracks to follow.

I've been in the process of disassembling a part of the firware to look for
these default settings as well as how to activate the power meter. This latter
was in fact already activated (but with 3dB resolution, since A107 had no
U12/CR3 populated).

.. _discussion: https://www.eevblog.com/forum/testgear/eip-545b-frenquency-counter
.. _`eevblog forum`: https://www.eevblog.com/forum/


Power Meter
===========

While I was waiting for the parts I was missing to modify the A107 as an option
02 enabled one, I was playing with the counter, and I discovered that the PM
was in fact already activated.

Obviously, there was no need for the local EPROM (U20) on A107 (with its 2
companions, U19 and U21) for the EIP454B. I already noticed the address range
where this EPROM is located on the EIP545A (0x4000) is already filled with
code/data in the main firmware on the CPU board (A105).

So I added an AD7524 (U12, 8-bit DAC), removed R39 and installed an FH1100
equivalent (QSCH1245 ie. an HP5082-2835) diode as CR3.

After that, I could read (uncalibrated) power with the expected 0.1dBm
resolution:


.. image:: {filename}images/eip545b/pm_full.jpg
   :alt: Power Meter at full resolution

*On avance !*

Now I still need to figure how to calibrate the damn stuff... A
calibration procedure is quickly described in the service manual, but the
procedure it imply writing the calibration table in the local EPROM on A107.
Since this is not populated for the EIP545B, it must lay somewhere else.

That's where the magic of the wonderful eevblog comunity shine: HighPrecision_,
who happens to have serviced these kind of test gears for years, `gave me the
correct address`_ for the PM calibration table: 0x0810, in the EEPROM.

Much quicker than finding this in the firmware!

Now I need a decent power meter to be able to calibrate it, but one step at a
time...


.. _HighPrecision: https://www.eevblog.com/forum/profile/?u=116109
.. _`gave me the correct address`: https://www.eevblog.com/forum/testgear/eip-545b-frenquency-counter/msg1400163/#msg1400163
