========================================================
 HP8904A Multifunction Synthetizer Repair: 10MHz output
========================================================

:Author: David Douard
:Category: Electronics
:Tags: HP8904A, repair, test equipment, signal generator

After having `fixed the PSU of one of my HP8904A`_ signal generator, I
discovered that the other unit had its 10MHz reference output
dead flat.

I've disassembled the main logic board, but unfortunately, the
schematic of this later A2 board (as it is referenced in the servce
manual) is notavailable in any available HP's manual...

The board I have is the second revision:

.. image:: {filename}images/hp8904a/A2_top.jpg
   :alt: The logic board (A2) of the HP8904A signal generator.

And the bottom side of the PCB:

.. image:: {filename}images/hp8904a/A2_bottom.jpg
   :alt: Bottom side of the A2 board.

According to the presence of soldering flux, it looks like the U46
chip (a 74ALS73CN) on this board has been replaced:
	 
.. image:: {filename}images/hp8904a/A2_U46.jpg
   :alt: The U46 chip seems to have been replaced.

After having moved my scope probe around the 10MHz output (J102), I've
found that the most probable culprit is the Q106 transistor (which
seems to be a bipolar one). The 10MHz arrives to the base signal, the
emitter is grounded, but nothing on the collector...

Unfortunately, HP had the awful habit of taging most of the parts in
their test equipments with custom references, even if most of them are
in fact regular parts.

The problem was then to identify a reasonable replacement part for
this puppy. It presents itself as a Motorola with weird reference
``3 0659``:

.. image:: {filename}images/hp8904a/HP8904A_Q106.jpg
   :alt: The failing transistor.
      
Having no luck searching the net, I've asked the `wonderful EEVBlog
community`_ for some help identifying this transistor. My question
obviously was answered very quickly by several fellows. First I've had
the correct reference for the transistor. Its HP part number is in
fact 1853-0659 (notice the 3-0659 as stamped on the transistor case),
and it is i fact a simple 2N3906.

But another forum member also noted that a wire was broken, as it is
clearly visible on the picture above.

So I did a very quit fix for this problem by simply resoldering the
broken leg of the transistor, and bingo, the 10MHz output is working
again!

This EEVBlog community really is awesome!

.. _`fixed the PSU of one of my HP8904A`: {filename}/hp8904a.rst
.. _`wonderful EEVBlog community`: http://www.eevblog.com/forum/repair/repair-of-an-hp8904a-signal-generator


